(export (version D)
  (design
    (source /home/mdchaparror/Documentos/balancing_robot/PCB/balancing_pcb/balancing_pcb.sch)
    (date "dom 13 ene 2019 17:56:19 -05")
    (tool "Eeschema 5.0.2-bee76a0~70~ubuntu18.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source balancing_pcb.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U1)
      (value "NodeMCU_1.0_(ESP-12E)")
      (footprint "ESP8266:NodeMCU1.0(12-E)")
      (libsource (lib ESP8266) (part "NodeMCU_1.0_(ESP-12E)") (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C3BC25F)))
  (libparts
    (libpart (lib ESP8266) (part "NodeMCU_1.0_(ESP-12E)")
      (fields
        (field (name Reference) U)
        (field (name Value) "NodeMCU_1.0_(ESP-12E)"))
      (pins
        (pin (num 1) (name "A0(ADC0)") (type input))
        (pin (num 2) (name RSV) (type input))
        (pin (num 3) (name RSV) (type input))
        (pin (num 4) (name "SD3(GPIO10)") (type BiDi))
        (pin (num 5) (name "SD2(GPIO9)") (type BiDi))
        (pin (num 6) (name "SD1(MOSI)") (type BiDi))
        (pin (num 7) (name "CMD(CS)") (type BiDi))
        (pin (num 8) (name "SDO(MISO)") (type BiDi))
        (pin (num 9) (name "CLK(SCLK)") (type BiDi))
        (pin (num 10) (name GND) (type input))
        (pin (num 11) (name 3.3V) (type power_out))
        (pin (num 12) (name EN) (type input))
        (pin (num 13) (name RST) (type input))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name VIN) (type power_in))
        (pin (num 16) (name 3.3V) (type power_out))
        (pin (num 17) (name GND) (type power_in))
        (pin (num 18) (name "TX(GPIO1)") (type BiDi))
        (pin (num 19) (name "RX(DPIO3)") (type BiDi))
        (pin (num 20) (name "D8(GPIO15)") (type BiDi))
        (pin (num 21) (name "D7(GPIO13)") (type BiDi))
        (pin (num 22) (name "D6(GPIO12)") (type BiDi))
        (pin (num 23) (name "D5(GPIO14)") (type BiDi))
        (pin (num 24) (name GND) (type power_in))
        (pin (num 25) (name 3.3V) (type power_out))
        (pin (num 26) (name "D4(GPIO2)") (type BiDi))
        (pin (num 27) (name "D3(GPIO0)") (type BiDi))
        (pin (num 28) (name "D2(GPIO4)") (type BiDi))
        (pin (num 29) (name "D1(GPIO5)") (type BiDi))
        (pin (num 30) (name "D0(GPIO16)") (type BiDi)))))
  (libraries
    (library (logical ESP8266)
      (uri /home/mdchaparror/Documentos/balancing_robot/PCB/balancing_pcb/librerias/ESP8266.lib)))
  (nets
    (net (code 1) (name "Net-(U1-Pad22)")
      (node (ref U1) (pin 22)))
    (net (code 2) (name "Net-(U1-Pad29)")
      (node (ref U1) (pin 29)))
    (net (code 3) (name "Net-(U1-Pad19)")
      (node (ref U1) (pin 19)))
    (net (code 4) (name "Net-(U1-Pad28)")
      (node (ref U1) (pin 28)))
    (net (code 5) (name "Net-(U1-Pad18)")
      (node (ref U1) (pin 18)))
    (net (code 6) (name "Net-(U1-Pad27)")
      (node (ref U1) (pin 27)))
    (net (code 7) (name "Net-(U1-Pad17)")
      (node (ref U1) (pin 17)))
    (net (code 8) (name "Net-(U1-Pad26)")
      (node (ref U1) (pin 26)))
    (net (code 9) (name "Net-(U1-Pad16)")
      (node (ref U1) (pin 16)))
    (net (code 10) (name "Net-(U1-Pad25)")
      (node (ref U1) (pin 25)))
    (net (code 11) (name "Net-(U1-Pad15)")
      (node (ref U1) (pin 15)))
    (net (code 12) (name "Net-(U1-Pad24)")
      (node (ref U1) (pin 24)))
    (net (code 13) (name "Net-(U1-Pad14)")
      (node (ref U1) (pin 14)))
    (net (code 14) (name "Net-(U1-Pad23)")
      (node (ref U1) (pin 23)))
    (net (code 15) (name "Net-(U1-Pad13)")
      (node (ref U1) (pin 13)))
    (net (code 16) (name "Net-(U1-Pad1)")
      (node (ref U1) (pin 1)))
    (net (code 17) (name "Net-(U1-Pad12)")
      (node (ref U1) (pin 12)))
    (net (code 18) (name "Net-(U1-Pad21)")
      (node (ref U1) (pin 21)))
    (net (code 19) (name "Net-(U1-Pad11)")
      (node (ref U1) (pin 11)))
    (net (code 20) (name "Net-(U1-Pad30)")
      (node (ref U1) (pin 30)))
    (net (code 21) (name "Net-(U1-Pad20)")
      (node (ref U1) (pin 20)))
    (net (code 22) (name "Net-(U1-Pad10)")
      (node (ref U1) (pin 10)))
    (net (code 23) (name "Net-(U1-Pad9)")
      (node (ref U1) (pin 9)))
    (net (code 24) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 25) (name "Net-(U1-Pad7)")
      (node (ref U1) (pin 7)))
    (net (code 26) (name "Net-(U1-Pad6)")
      (node (ref U1) (pin 6)))
    (net (code 27) (name "Net-(U1-Pad5)")
      (node (ref U1) (pin 5)))
    (net (code 28) (name "Net-(U1-Pad4)")
      (node (ref U1) (pin 4)))
    (net (code 29) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 30) (name "Net-(U1-Pad2)")
      (node (ref U1) (pin 2)))))