(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu18.04.1)

  (general
    (thickness 1.6)
    (drawings 4)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 31)
  )

  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )

  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )

  (net 0 "")
  (net 1 "Net-(U1-Pad1)")
  (net 2 "Net-(U1-Pad2)")
  (net 3 "Net-(U1-Pad3)")
  (net 4 "Net-(U1-Pad4)")
  (net 5 "Net-(U1-Pad5)")
  (net 6 "Net-(U1-Pad6)")
  (net 7 "Net-(U1-Pad7)")
  (net 8 "Net-(U1-Pad8)")
  (net 9 "Net-(U1-Pad9)")
  (net 10 "Net-(U1-Pad10)")
  (net 11 "Net-(U1-Pad11)")
  (net 12 "Net-(U1-Pad12)")
  (net 13 "Net-(U1-Pad13)")
  (net 14 "Net-(U1-Pad14)")
  (net 15 "Net-(U1-Pad15)")
  (net 16 "Net-(U1-Pad16)")
  (net 17 "Net-(U1-Pad17)")
  (net 18 "Net-(U1-Pad18)")
  (net 19 "Net-(U1-Pad19)")
  (net 20 "Net-(U1-Pad20)")
  (net 21 "Net-(U1-Pad21)")
  (net 22 "Net-(U1-Pad22)")
  (net 23 "Net-(U1-Pad23)")
  (net 24 "Net-(U1-Pad24)")
  (net 25 "Net-(U1-Pad25)")
  (net 26 "Net-(U1-Pad26)")
  (net 27 "Net-(U1-Pad27)")
  (net 28 "Net-(U1-Pad28)")
  (net 29 "Net-(U1-Pad29)")
  (net 30 "Net-(U1-Pad30)")

  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(U1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad14)")
    (add_net "Net-(U1-Pad15)")
    (add_net "Net-(U1-Pad16)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad20)")
    (add_net "Net-(U1-Pad21)")
    (add_net "Net-(U1-Pad22)")
    (add_net "Net-(U1-Pad23)")
    (add_net "Net-(U1-Pad24)")
    (add_net "Net-(U1-Pad25)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad28)")
    (add_net "Net-(U1-Pad29)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
  )

  (module "ESP8266:NodeMCU1.0(12-E)" (layer F.Cu) (tedit 5AF3DDCB) (tstamp 5C5EF3C8)
    (at 172.72 80.01)
    (path /5C3BC25F)
    (fp_text reference U1 (at 0 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text value "NodeMCU_1.0_(ESP-12E)" (at 0 -5.08) (layer F.Fab)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 13.98 24.13) (end 3.81 24.13) (layer F.SilkS) (width 0.15))
    (fp_text user USB (at 0 22.86) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user "RF Antenna" (at 0 -20.32) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_line (start 5.5 -17) (end -5.5 -17) (layer F.SilkS) (width 0.15))
    (fp_line (start 5.5 -24.13) (end 5.5 -17) (layer F.SilkS) (width 0.15))
    (fp_line (start -5.5 -17) (end -5.5 -24.13) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 25.13) (end -3.8 19.4) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 19.4) (end 3.8 19.4) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 19.4) (end 3.8 25.13) (layer F.SilkS) (width 0.15))
    (fp_line (start 3.8 25.13) (end -3.8 25.13) (layer F.SilkS) (width 0.15))
    (fp_arc (start -13.97 -22.86) (end -15.24 -22.86) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start 13.97 -22.86) (end 13.97 -24.13) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start 13.97 22.86) (end 15.24 22.86) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_arc (start -13.97 22.86) (end -13.97 24.13) (angle 90) (layer F.SilkS) (width 0.15))
    (fp_line (start 15.24 -22.86) (end 15.24 22.86) (layer F.SilkS) (width 0.15))
    (fp_line (start -15.24 -22.86) (end -15.24 22.86) (layer F.SilkS) (width 0.15))
    (fp_line (start -3.8 24.13) (end -13.97 24.13) (layer F.SilkS) (width 0.15))
    (fp_text user VIN (at -11.43 17.78) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user G (at -11.43 15.24) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user RST (at -11.43 12.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user EN (at -11.43 10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user 3V (at -11.43 7.62) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user G (at -11.43 5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user SK (at -11.43 2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user SO (at -11.43 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user SC (at -11.43 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user S1 (at -11.43 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user S2 (at -11.43 -7.62) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user S3 (at -11.43 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user VU (at -11.43 -12.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user G (at -11.43 -15.24) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user A0 (at -11.43 -17.78) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user 3V (at 11.43 17.78) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user G (at 11.43 15.24) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user TX (at 11.43 12.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user RX (at 11.43 10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D8 (at 11.43 7.62) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D7 (at 11.43 5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D6 (at 11.43 2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D5 (at 11.43 0) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user G (at 11.43 -2.54) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user 3V (at 11.43 -5.08) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D4 (at 11.43 -7.62) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D3 (at 11.43 -10.16) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D2 (at 11.43 -12.7) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D1 (at 11.43 -15.24) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_text user D0 (at 11.43 -17.78) (layer F.SilkS)
      (effects (font (size 1 1) (thickness 0.15)))
    )
    (fp_circle (center 12.7 21.59) (end 13.97 20.32) (layer F.SilkS) (width 0.15))
    (fp_circle (center -12.7 21.59) (end -11.43 20.32) (layer F.SilkS) (width 0.15))
    (fp_circle (center -12.7 -21.59) (end -11.43 -22.86) (layer F.SilkS) (width 0.15))
    (fp_circle (center 12.7 -21.59) (end 13.97 -22.86) (layer F.SilkS) (width 0.15))
    (fp_line (start 13.97 -24.13) (end -13.97 -24.13) (layer F.SilkS) (width 0.15))
    (pad 1 thru_hole circle (at -13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(U1-Pad1)"))
    (pad 2 thru_hole circle (at -13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(U1-Pad10)"))
    (pad 11 thru_hole circle (at -13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(U1-Pad11)"))
    (pad 12 thru_hole circle (at -13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(U1-Pad14)"))
    (pad 15 thru_hole circle (at -13.97 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(U1-Pad15)"))
    (pad 16 thru_hole circle (at 13.97 17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(U1-Pad16)"))
    (pad 17 thru_hole circle (at 13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(U1-Pad17)"))
    (pad 18 thru_hole circle (at 13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(U1-Pad20)"))
    (pad 21 thru_hole circle (at 13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(U1-Pad21)"))
    (pad 22 thru_hole circle (at 13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 22 "Net-(U1-Pad22)"))
    (pad 23 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(U1-Pad23)"))
    (pad 24 thru_hole circle (at 13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 24 "Net-(U1-Pad24)"))
    (pad 25 thru_hole circle (at 13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(U1-Pad25)"))
    (pad 26 thru_hole circle (at 13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 26 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 27 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at 13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad28)"))
    (pad 29 thru_hole circle (at 13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad29)"))
    (pad 30 thru_hole circle (at 13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad30)"))
  )

  (gr_line (start 139.7 114.3) (end 139.7 38.1) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 114.3) (end 139.7 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 203.2 38.1) (end 203.2 114.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.7 38.1) (end 203.2 38.1) (layer Edge.Cuts) (width 0.15))

)
